

Budapest University of Technology and Economics

Faculty of Electrical Engineering and Informatics

Department of Control Engineering and Information Technology

Areeba Tabassum Shoaib

MAXIMIZING POWER CONSUMPTION OF MIMO NETWORK USING A NOVEL QUANTUM GENETIC ALGORITHM

SUPERVISOR

Dr. El Gaily Sara

BUDAPEST, 2023

Contents

[Summary 4](#_Toc129318126)

[Sommaire 5](#_Toc129318127)

[Acknowledgement 6](#_Toc129318128)

[1 Introduction 7](#_Toc129318129)

[1.1 Quantum Computing Overview 7](#_Toc129318130)

[1.1.1 Postulates of Quantum Computing 7](#_Toc129318131)

[1.1.2 Quantum Entanglement 10](#_Toc129318132)

[1.1.3 No-cloning theorem 12](#_Toc129318133)

[1.1.4 Quantum Teleportation 12](#_Toc129318134)

[1.1.5 Quantum Parallelism 13](#_Toc129318135)

[1.1.6 Grover’s Algorithm 14](#_Toc129318136)

[1.2 Overview about MIMO System 15](#_Toc129318137)

[1.3 Overview about Genetic Algorithms 17](#_Toc129318138)

[1.4 Overview about Quantum Genetic Algorithm 17](#_Toc129318139)

[1.4.1 Program codes 18](#_Toc129318140)

[1.4.2 References 18](#_Toc129318141)

[2 Last operations and checks 19](#_Toc129318142)

[References 20](#_Toc129318143)

[Annex 21](#_Toc129318144)

STUDENT DECLARATION

I, **Areeba Tabassum Shoaib**, the undersigned, hereby declare that the present BSc/ thesis work has been prepared by myself and without any unauthorized help or assistance. Only the specified sources (references, tools, etc.) were used. All parts taken from other sources word by word, or after rephrasing but with identical meaning, were unambiguously identified with explicit reference to the sources utilized.

I authorize the Faculty of Electrical Engineering and Informatics of the Budapest University of Technology and Economics to publish the principal data of the thesis work (author's name, title, abstracts in English and in a second language, year of preparation, supervisor's name, etc.) in a searchable, public, electronic and online database and to publish the full text of the thesis work on the internal network of the university (this may include access by authenticated outside users). I declare that the submitted hardcopy of the thesis work and its electronic version are identical.

Full text of thesis works classified upon the decision of the Dean will be published after a period of three years.

Budapest, 9 March 2023

...…………………………………………….

Areeba Tabassum Shoaib

Summary

Quantum computing is one of the most promising approaches to addressing the problems of computational complexity, data storage, and power consumption because of its extremely fast performance. Applying the principles of quantum computing to the development of optimization algorithms is a rapidly growing field of study.

With its ability to provide game-changing improvements in area throughput and energy efficiency, the massive multiple-input multiple-output (MIMO) system offers significant potential for 5th generation (5G) wireless communication systems. The number of antennas used by the base station is increased in massive MIMO. This has several advantages, including an array gain that may be utilized to expand coverage, favorable propagation that makes user separation easier, and channel hardening that makes the system more robust and stable. Yet, the computational complexity of the embedded optimization techniques in MIMO systems remains a problem. Several techniques, such as the Nash equilibrium-based effective water-filling algorithm (WFA), have been developed in an effort to enhance the power allocation system for MIMO.

This thesis focuses on the question of how the power consumption of MIMO systems can be maximized by using a novel Quantum Genetic Algorithm.

In this research , we implemented a quantum optimization technique known as the Quantum Extreme Value Searching Algorithm (QEVSA) to Develop a new Unconstrained Quantum Genetic Algorithm (UQGA). Not Completed!!!

Sommaire

The text of a ½-1 page long summary goes here in a second language, different of English (German, French, Portuguese, Russian, Finnish, Korean, Chinese, Japanese, Hungarian, etc,). This summary is the translation of the summary in English and has to be also uploaded to the Thesis Portal separately.

Acknowledgement

# Introduction

This chapter presents a couple of examples of the usual formatting requirements of different items you may need to include into your thesis.

## Quantum Computing Overview

In classical computing, the smallest unit of information is referred to as a "bit" and can be represented by one of two states, "0" or "1"; these states are also known as classical states. The classical processor carries out a variety of transformations on classical states, i.e., information processing using classical gates. Comparable to classical computing, Quantum computing employs specific quantum elements that do not exist in traditional computation. It is important to note that there are four primary postulates that describe quantum computer, and they are as follows:

### Postulates of Quantum Computing

**First postulate (State-space)**

A qubit is the fundamental quantum systems unit in the quantum universe that can simultaneously contemplate both classical states, referred as superposition. Below is an illustration of a qubit:

(

where a and b are complex coefficients, and |0 > and |1 > are the so-called computational basis states , such that,

Two classical states can coexist in one qubit. The outcome of a coin flip can be thought of as an example of a qubit. If we toss a coin (and assume it's fair), we've got an equal chance of getting a head or a tail with a probability of 0.5 for either outcome.

It is important to stress that is a superposition of two states, and the precise formula of (1.1) can be stated as follows:

**Second postulate (Evolution)**

How a quantum state changes over time is described by the second postulate. For those unfamiliar, the quantum gate is just a unitary operator used in quantum computing.

A unitary operator satisfies the following formula:

Moreover, the unit norm of the quantum state is conserved by a unitary transformation. The relation between and is shown as in Figure 1.1, where between is an input quantum state and is the output quantum state after performing the unitary transform U.

Logic gates in digital circuits function similarly to quantum gates in quantum circuits. The manipulation and alteration of qubits is their primary goal. Contrary to logic gates, quantum gates support the idea of reversibility, which allows us to easily convert an input quantum state into an output quantum state and vice versa.

We list some well-known quantum gates here that work with just one qubit,

**Hadamard-gate**

All quantum algorithms rely heavily on this operator during their startup phase. It is well known that when the Hadamard gate is dominated by classical states, uniform probability distributions of all computational basis states are generated.

**Third postulate (Measurement)**

It is important to note that a quantum state cannot be observed; the only way to ascertain its state is to carryout a measurement. Notice that the measurement of a quantum system can be characterized by measurement operators , where m represents a potential measurement outcome. If the system is in state , then the probability of measuring the potential state m may very well be expressed as:

where the adjoint of is denoted by and the adjoint of is denoted by . The measurement apparatus is viewed as a connection between the classical and quantum worlds; hence, in order to validate the precision of the constructed measurement apparatus, the following completeness relationship needs to be satisfied.

**Fourth postulate (Composite systems)**

The postulate describes a quantum register. The term "quantum register" refers to the component that is created when numerous quantum states are grouped together using a mathematical technique called the "tensor product." Take, for instance, the case where there are three qubits available. In order to combine these three qubits into a single quantum register, we will make use of the tensor product.

The first qubit can be represented in the following manner:

While the second and third qubits are respectively described as,

It is possible to achieve the composite of these three qubits in the following manner:

### Quantum Entanglement

Quantum entanglement was first discovered in the 1960s and was named after John von Neumann, who discovered quantum mechanics. Quantum entanglement is a logical connection between quantum states in such a way that they are spatially separated but communicating with each other; in other words, there is a certain hidden relationship between the quantum states.. For instance, if two quantum states are separated by a significant distance, the measurement of one quantum state enables instantaneous estimations of the other quantum state. The capacity of quantum entanglement to communicate at speeds greater than the speed of light is perhaps its most crucial function, as it will greatly accelerate the rate at which human society expands.

The most well-known piece of mathematical equipment that can generate entangled states is called a CNOT-gate. One of the inputs of the CNOT gate is used for controlling the device, and the other input is used for feeding it data. One will be used for the output control, while the other will be used for the output data. When we input 0 into the control terminal, the value at the data terminal does not change, which is a crucial point to keep in mind. If we enter 1 into the control terminal, then the value at the data terminal will be averted. For example, if our control terminal is set to 1, and the data terminal is receiving input 1, then the output of the data terminal will be 0.

It is worth noting that the most well-known entangled states are termed Bell states, and they are stated as follows:



Both the Hadamard Gate and the CNOT Gate can be used to produce them. The circuit that produces a Bell state is illustrated in the figure below.

**H**

.

The circuit depicted in Figure 1.2 is responsible for the generation of four distinct entangled pairs of "Bell states." The following is a list of them in order of precedence:

### No-cloning theorem

According to the no-cloning theorem, it is not possible to clone unknown quantum states in the universe of quantum mechanics. However, it is possible to clone either recognized quantum states as well as orthogonal quantum states. Due to the fact that identical backups of quantum states cannot be created in advance in quantum computing, the "no-cloning theorem" rules out the use of conventional error correcting techniques on quantum states. Let's offer an example. Consider for a moment that there are two possible quantum states: |0> and |1>. It is not difficult to check whether or not the inner product of these two states is equal to zero. As a result, the quantum states 0 and 1 are orthogonal to one another. We are consequently able to clone them. Because of the no-cloning theorem, it is impossible to fix errors in quantum states by using the more conventional methods that were previously utilized. There is no way to build backup copies on the quantum states in the middle of the computation and check for mistakes in those copies.

The no-cloning theorem can be useful in a variety of situations. For example, quantum key distribution (QKD) is a method of communicating between two parties that is safer and more secure because it does not rely on cloning power (the generated key cannot be cloned by eavesdroppers). PROOF??

### Quantum Teleportation

The power of quantum entanglement is utilized in the process of quantum teleportation in order to swiftly transport an object from one location to another. The theory of quantum teleportation has been proven, but there are still a lot of obstacles to overcome before it can be used in practice. It is an interesting fact to note that the capabilities afforded by quantum teleportation have been employed as the primary concept for quantum repeaters and communication channels.

The construction of a quantum teleportation apparatus can often be accomplished in one of two ways. The first method involves reducing the size of the object by breaking it up into more manageable pieces, such as fundamental particles like electrons and protons. After that, they are sent through a communication channel that uses quantum mechanics. After that, we move on to finish reassembling them on the opposite cabinet. The fact that a quantum error correction is necessary is the most significant disadvantage of pursuing this technique. The classical communication channel is used in place of the quantum communication channel in the second technique (the classical information is delivered). One of the limitations of this method is that it does not eliminate the need to measure the states of all the collected particles. Let's say that Alice and Bob want to transport just one qubit between their two locations. They have to carry out a sequence of procedures. The first thing that needs to be done is for Alice and Bob to split their a bell pair. After that, Alice needs to do a variety of operations on her qubits (CNOT and Hadamard, etc.). At long last, she is obligated to carry out a measurement. After that, the result that was produced is then communicated to Bob through the traditional way. Last but not least, Bob may retrieve the initial qubit (the qubit that was transmitted by Alice) by making use of either the I gate, the ZX gate, the X gate, or the Z gate.

### Quantum Parallelism

The concept of quantum parallelism is regarded as the fundamental building block of any quantum computation. It permits the execution of activities that have a significantly lower computational complexity than the one that has traditionally been used. Let's say that we have a function that has n inputs but only one output. With the traditional approach, we need 2n-1 steps to get back the output result, while the quantum parallelism strategy just needs one step from us O(1).

A unique quantum gate, known as an f controlled CNOT gate, is responsible for carrying out the quantum parallelism. This gate is formulated as follows:

The following describes the output function obtained by applying the f-controlled CNOT gate:

As can be seen, the evaluation of each and every x is performed in a single step by the function f. The most significant shortcoming is that we are unable to verify the values of any f(x) due to the fact that the measurement equipment returns just a single value. Applying an amplification amplitude so that the probability of the desired outcome reaches one is the approach that needs to be taken in order to solve this challenge.

### Grover’s Algorithm

To be done!!!

## Overview about MIMO System

There has been a significant leap forward in communication technology ever since Marconi conducted his first experiments in the late 1800s, a fascination in the opportunities presented by wireless communications. Since then, wireless technology has progressed. The connections that once could only send data at a sluggish and irregular rate have evolved into the high-capacity networks that we see in use today. Numerous fields of application can be found: voice services have become so widespread that they can frequently take the place of fixed line services; wireless local area networks are up and running in many residential, office, municipal, or school buildings; and personal area networks, such as Bluetooth links, form wireless connections between various consumer electronics devices. In spite of this, there is a seemingly incessant drive to enhance the capabilities of wireless communications in terms of throughput and/or reliability. Furthermore, there are a wide variety of novel applications and environments for which wireless technology is envisioned. But, despite the continually increasing number of wireless applications, bandwidth is still a very scarce resource, just as it was back in the days of Marconi.

The limitation in available bandwidth has driven the development of unique transmission strategies. Out of these novel transmission techniques, multiple-input multiple-output (MIMO) systems have gained a lot of research interest in recent years.

MIMO is an abbreviation that stands for "Multiple Input Multiple Output." This abbreviation describes a method of wireless communication known as MIMO, which makes use of multiple antennas at both the transmitter and the receiver to increase the system's overall performance. The basic purpose of multiple input multiple output, or MIMO, systems is to improve the quality of communication while simultaneously expanding the capacity of wireless communication channels. Multi-input, Multi-output (MIMO) systems include several antennas at both ends of the communication link. The rank of a MIMO system is defined by the total number of antennas. Two broadcast antennas and two receive antennas are used in a 2x2 MIMO system. Multiple-input multiple-output (MIMO) systems allow the transmitter to convey numerous data streams at once by making use of multiple antennas. The numerous antennas at the receiving end pick up this information since it has been mixed with other streams before transmission. The original data is separated into its component streams and recovered by the receiver using signal processing techniques.

Spatial multiplexing, diversity techniques, beamforming, and interference cancellation are just a few of the methods that MIMO systems can employ to boost the efficiency of wireless communication channels. When transmitting several data streams, diversity approaches use various antennas to mitigate the effects of fading and other signal impairments, while spatial multiplexing is a technique that uses multiple antennas to do the same. Beamforming uses a network of antennas to concentrate a signal in one location, while interference cancellation eliminates noise in the received signal.

Diagram

Description automatically generatedMIMO technology can make a big difference in the system's speed, coverage area, and quality of service (QoS). Using MIMO, the best way to send data depends on how the antenna arrays in the sender and receiver are set up. In general, optimizing is a hard and expensive job. So, scientists and engineers have come up with effective ways to optimize MIMO projects so that they can be useful and affordable. In the Cellular Mobile System (CMS), algorithms based on artificial intelligence are used to optimize the way data is sent .

Multiple-input multiple-output (MIMO) link, in which the transmitting base station directs three separate spatial beams at the receiver.

## Overview about Genetic Algorithms

## Overview about Quantum Genetic Algorithm

All images must have captions. It is advised to add captions by right clicking on the image and selecting the *Insert Caption …* command. The resulting caption will have automatically **Caption** style and you are required to specify the caption details in a dialog window.



1.2. figure: Caption example

### Program codes

Use the **Prg code** syle to insert programming code as bellow.

using System;

namespace MyApp

{

class Program

{

static void Main( string[] args )

{

Console.WriteLine( "Hello world! Kachi Kapsida" );

}

}

}

### References

Items in the reference list are formatted using the **Reference item** style so that the titles are emphasized by the **Reference source** style.

You may place citations of references in the text using the *Insert / Cross-reference* command (an example looks like this: [1]). These citations are updated automatically if a new reference is added or their order is changed.

# Last operations and checks

Once the content is ready, you should not forget the following operations:

* Update cross-references: select all the text first (Ctrl+A) and then press F9 to let the Word to update all cross-references. A check for “Error!..” at the places of references should be carried out.
* Specify document properties: you need to specify all necessary meta-data for the document such as the author, title, keywords, etc. The Document property panel appears if the File / Info / Document panel command is selected and these properties can be set there.
* Check the PDF: the best test of the document is to go through the PDF file generated from the Word version attentively.

References

1. Levendovszky, J., Jereb, L., Elek, Zs., Vesztergombi, Gy.: Adaptive statistical algorithms in network reliability analysis, Performance Evaluation - Elsevier, Vol. 48, 2002, pp. 225-236
2. National Istruments: LabVIEW grafikus fejlesztői környezet leírása, <http://www.ni.com/> (2010. nov.)
3. Fowler, M.: UML Distilled, 3rd edition, ISBN 0-321-19368-7, Addison-Wesley, 2004
4. Wikipedia: Evaluation strategy, <http://en.wikipedia.org/wiki/Evaluation_strategy> (revision 18:11, 31 July 2012)

Annex